**Alcuni dei principali lavori che sono stati realizzati con il supporto del Laboratorio**

**Some related papers where Thermal Analysis was used**

Tateo, F., Cortecci, G., Minguzzi, V., & Morandi, N. (2001). Mineralogy and geochemistry of early-formed deep marine dolomite in the Castagnola Formation (Oligocene-Miocene, Northern Italy). European Journal of Mineralogy, 13(4), 727-741.

Sabetta, T., Bargossi, G.M., D'Amico, C., Grillini, G.C., & Minguzzi, V. (2001). Sandstones, mortars and clay bricks from Palazzo Fava in Bologna (Italy): A mineralogical petrographic study. GeoActa, 1, 71-82.

Dellisanti, F., Minguzzi, V., & Morandi, N. (2001). Experimental results from thermal treatment of asbestos containing materials. GeoActa, 1, 61-70.

Morandi, N., Minguzzi, V., Tateo, F., & De Carlo, M. (1999). Incipient vermiculitization processes in biotites from Italian oligo-miocene sediments. Mineralogica et Petrographica Acta, 42, 29-40.

Minguzzi, V., Morandi, N., Tagnin, S., Tateo, F. (1999). Composition and properties of clay used in thermal centres in Emilia-Romagna. Mineralogica et Petrographica Acta, 42, 287-298.

Dellisanti, F., Calafato, A., Pini, G.A., Moro, D., Ulian, G., & Valdrè, G. (2018). Effects of dehydration and grinding on the mechanical shear behaviour of Ca-rich montmorillonite. Applied Clay Science, 152, 239-248.

Dellisanti, F., & Valdre, G. (2012). The role of microstrain on the thermostructural behaviour of industrial kaolin deformed by ball milling at low mechanical load. International Journal of Mineral Processing, 102-103, 69-77.

Dellisanti, F., Minguzzi, V., & Valdre, G. (2011). Mechanical and thermal properties of a nanopowder talc compound produced by controlled ball milling. Journal of Nanoparticle Research, 13, 5919-5926.

Dellisanti, F., & Valdre, G. (2010). On the high-temperature structural behaviour of talc (Mg3Si4O10(OH)2) to 1600 °C: Effect of mechanical deformation and strain. Philosophical Magazine, 90(17-18), 2443-2457.

Dellisanti, F., & Valdre, G. (2008). Linear relationship between thermo-dehydroxylation and induced-strain by mechanical processing in vacuum: The case of industrial kaolinite, talc and montmorillonite. International Journal of Mineral Processing, 88(3-4), 94-99.